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AUTOMATIC SLIDING ENTRANCES
HD-Slide® Series 2001 Ballistic Resistant 6” x 8” Header
Sliding Door System with Electric Belt Drive Operator | AB2.02

	[bookmark: _Hlk152857433]Specification
	Selection

	Door ID
	to be selected/edited by specifier

	Product Name
	HD-Slide® Series 2001 Ballistic Resistant 6” x 8” Header

	Design
	Bi-parting - Perimeter mounted within rough opening with sliding panel(s) sliding along sidelite.

	Breakout
	Type 110: Slide-swing panel(s) ‘SX’ shall slide along exterior side.

	Height
	Edit Section 2.02 Section A. Standard: 7’ 6 specifiable. Transom: Specifiable.

	Width
	Edit Section 2.02 Section A. Standard: Singles 7’ – 9’; Bi-parting: 8’ – 16’.

	Finish
	Edit Section 2.02.05 Section B

	Door Panel Materials
	Aluminum: 0.125” thick

	Stiles
	Medium stile construction: 3 3/4” (95mm) wide

	Jamb Dimension
	1 3/4" (44mm) deep x 4 (104 mm) high

	Muntin
	Edit Section 2.02.03. Section C.2

	Bottom Rail
	Edit Section 2.02.03. Section C.3

	Threshold
	1/2” (13mm) tall by 7” (178mm) wide

	Header Size
	6” x 8”

	Drive System
	1/4 HP DC permanent magnet motor with heavy duty worm gear transmission
Electromechanical | Belt Driven

	Activation/Safety Sensors
	Automatic Operation Sensor System Compliant with ANSI A156.10

	Power Fail Option
	Edit Section 2.02.03. Section I

	Automatic Lock Option
	Edit Section 2.02.03. Section G.2

	Locking
	Standard Lock - 2-Point Locking

	Max Door Panel Weight
	Up to 300 lbs.

	Glazing Prep
	1” UL752 BR-3 rated glass as specified by the manufacturer

	Voltage
	Section 2.02.02 Section A.8

	Temperature Rating
	-30°F to 130°F

	Codes & Standards
	ANSI Z97.1, ANSI A117.1, ANSI/BHMA A156.10, ANSI A156.38, ANSI A156.5, NFPA 101, NFPA 70, ASTM B221, ASTM B209, AAMA 611, AAMA 701, ICC/IBC, BOCA, ICBO/UBC, UL 325, UL 752 ISO 9001, AA, NAAMM, AAADM



These specifications represent the exacting selection you have made for your project [PROJECT], including door configuration, colors and options and depict design features that are commonly used. Horton Automatics will custom manufacture each product to these specifications. It is the customer’s responsibility to validate that each configuration is suitable for the intended application. All specifications and designs contained herein are subject to change without notice or obligation. Consult www.hortondoors.com’ spec desk at 1-800-531-3111 or specs@hortondoors.com for assistance.




DIVISION 08 - OPENINGS
SECTION 08 42 29.23 SLIDING AUTOMATIC ENTRANCES
PART I – GENERAL

1.01 SUMMARY
A. WORK INCLUDED: 
Furnish specified complete automatic door system manufactured, fabricated & installed to meet manufacturer’s specifications and applicable codes at the time of purchase.
B. RELATED WORK:
1. Division 7 Sections for caulking to the extent not specified in this section.
2. Division 8 Sections for aluminum-framed entrances and storefronts for entrances furnished separately.
3. Division 8 Section "All-Glass Entrances and Storefronts" for entrances furnished separately.
4. Division 8 Section "Door Hardware" for hardware to the extent not specified in this Section.
5. Division 8 Section "Glazing" for materials and installation requirements of glazing for automatic entrances. 
6. Division 26 Sections for electrical connections provided separately including conduit and wiring for power to, and control of, automatic door operators.

[bookmark: _Hlk148367541]1.02 REFERENCES
A. American National Standards Institute (ANSI):
1. ANSI Z97.1: Safety Glazing Materials Used in Buildings - Methods of Test
2. ANSI A117.1: Accessible and Usable Buildings and Facilities
3. ANSI/BHMA A156.10: Power Operated Pedestrian Doors - Sliding Doors section
4. ANSI A156.38: Low Energy Power Operated - Sliding Doors section
5. ANSI A156.5: Standard for Auxiliary Locks and Associated Products
B. National Fire Protection Association (NFPA):
1. NFPA 101: Safety to Life from Fire in Buildings & Structures
2. NFPA 70: National Electrical Code
C. ASTM International:
1. ASTM B221: Aluminum-Alloy Extruded Bars, Rods, Shapes and Tubes
2. ASTM B209: Standard Specification for Aluminum and Aluminum Alloy Sheet and Plate
D. American Architectural Manufacturers Association (AAMA):
1. AAMA 611: Voluntary Specification for Anodized Architectural Aluminum
2. AAMA 701: Voluntary Specification for Pile Weatherstripping and Replaceable Fenestration Weatherseals
E. International Code Council (ICC): ICC/IBC: International Building Code
F. Building Officials and Code Administrators International (BOCA)
G. International Conference of Building Officials / Uniform Building Code (ICBO/UBC)
H. Electrical Testing Laboratory (ETL/UL): 
1. UL 325: Electrical Door, Drapery, Gate, Louver, and Window Operators and Systems.
2. UL 752: Bullet-Resisting Equipment
I. Intertek, Warnock Hersey (ETL): Testing Laboratory and Certification Agency joined with ETL SEMKO
J. International Organization for Standardization (ISO): ISO 9001: Quality Management Systems
K. Aluminum Association (AA): Aluminum Finishes Manual
L. National Association of Architectural Metal Manufacturers (NAAMM)
M. American Association of Automatic Door Manufacturers (AAADM)

DEFINITIONS
1. Activation Device: A device that, when actuated, sends an electrical signal to the door operator to activate the operation of the door.
2. Knowing Act: Consciously initiating the opening of a power-operated door using acceptable methods, including wall-mounted switches such as push plates and controlled access devices such as keypads, card readers, and key switches.
3. Safety Device: A tested system that works in conjunction with the automatic door control that detects the presence of a person or an object within a zone where contact could occur and provides a signal to stop the movement of the door.

1.03 SUBMITTALS
A. SHOP DRAWINGS & PRODUCT DATA 
1. Provide product data sheets including installation details, material descriptions, dimensions of individual components and profiles, fabrication, operational descriptions, and finishes.
2. Include plans, elevations, sections, details, hardware mounting heights, additional accessories, and attachments to other work. 
3. Submit drawings showing layout, profiles, product components including anchorage, accessories, finish, and glazing details (where required)
4. Samples: Color samples for selection of factory-applied color finishes will be provided as request.
5. Environmental & Sustainability Information: 
a. Environmental Product Declaration 
b. Manufacturer's product information and applicable sustainability program credits that are available towards a LEED rated product certification.
c. Credit MR 4.1 and 4.2: Manufacturer's or fabricator's certificate indicating percentage of post-consumer recycled content by weight and pre-consumer recycled content by weight for each product specified under this section.
6. AAADM Inspection & Reports:  AAADM inspection compliance form completed and signed by a certified AAADM inspector prior to doors being placed in operation as proof of compliance with ANSI A156.10 
B. CLOSEOUT SUBMITTALS: 
Owner’s Manual & Warranty document as specified herein. 
Operating and Maintenance Manuals: Provide manufacturers operating, owners and maintenance manuals for each item specified. Include the name, address, and contact information of the manufacturers providing the entrance and their nearest service representatives. The final copies should be delivered after completion of the installation test to include the spare parts list. 

1.04 QUALITY ASSURANCE
A. INSTALLERS QUALIFICATIONS: Installer shall be factory trained, certified by AAADM, and experienced in performing work of this section.

B. MANUFACTURER'S QUALIFICATIONS: 
1. Manufacturer to have minimum of (5) five years successful experience in the fabrication of automatic doors of the type required for this project. 
2. Manufacturer capable of providing field service representation during installation, approving acceptable installer, and approving the application method.

C. CERTIFICATIONS: Automatic sliding door systems and options shall be factory certified to meet performance design criteria in accordance with the following standards as applicable:
1. ANSI A156.10: For Power Operated Pedestrian Doors; Sliding Doors section.
2. NFPA 101: Code for Safety to Life from Fire in Buildings & Structures.
3. ETL Listed: Tested to UL 325 Standard.
4. BOCA: Means of Egress, Power Operated Doors
5. ICBO/UBC: Egress Through Lobbies
6. ICC/IBC: Egress Section 
7. CUL Approved for use in Canada 
8. UL 752: Bullet-Resisting Equipment 11th Edition Levels 1-3

D. PERFORMANCE REQUIREMENTS:
1. Operating Temperature Range: Capable of -30° F to 130° F (-34° C to 54° C).
2. Opening Force Requirements:
Slide-swing panels shall require no more than 50 lbf (222 N) of force to swing open. Slide-swing panels shall be capable of swinging out 90° from any position of slide movement.
3. Closing Force Requirements:
Maximum force required to prevent sliding panel from closing = 30 lbf (124.5 N) Adjustable Reversing Circuit will reopen door unit if closing path is obstructed 
4. Slide-swing panels and swing-out sidelites shall have torsion springs designed to re-close panel if pushed open in the direction of egress.
5. If power fails, slide panels can be manually slid open as per NFPA 101 or ICC/IBC. Continuous automatic operation would require unit to be powered by facility-provided UPS (Uninterrupted Power Source. 
6. Units with floor mounted track and breakaway feature are UL listed as an exit way and are compliant with NFPA 101.

1.05 PROJECT CONDITIONS
A. FIELD MEASUREMENTS:
Verify actual dimensions/openings by field measurements before fabrication and record on shop drawings. Coordinate with fabrication and construction schedules to avoid construction delays.

B. ON-SITE FIELD CONDITIONS REQUIRED PRIOR TO INSTALLATION:
1. Approved Shop drawings must be referenced and confirmed by the General Contractor before fabrication.
2. Opening must be verified to be plumb, straight, and secure.
3. It is the duty of the General Contractor to make the door installer aware of any nonconforming conditions or equipment as indicated on the shop drawings.
4. General Contractor is required to coordinate the layout and installation of the automatic door equipment in connection to power supplies.
5. Mounting Surfaces: General Contractor shall verify all surfaces to be plumb, straight, and secure; substrates to be of proper dimension and material.
6. General Contractor shall advise of any inadequate conditions or equipment.

1.06 DELIVERY, STORAGE AND HANDLING
A. ORDERING AND DELIVERY: Comply with factory's ordering instructions and lead time requirements. Delivery shall be in factory's original, unopened, undamaged containers with identification labels intact.

B. STORAGE AND PROTECTION: Provide protection from exposure to harmful weather conditions and vandalism

1.07 WARRANTIES
A. WARRANTY PERIOD: 2-year warranty: Labor & transportation costs covered for replacement of defective parts in material and workmanship from the Date of Substantial Completion.

B. DISTRIBUTOR'S WARRANTY: 1-year warranty: Labor & transportation charges for defective parts replacement 

C. SERVICE AND REPAIRS: 
1. During the warranty period, a factory-trained technician shall perform service and affect repairs.
2. A safety inspection shall be performed after each adjustment or repair, and a completed inspection form submitted to the owner.

D. WARRANTY WORK HOURS: During the warranty period, all warranty work shall be performed during normal working hours by our distribution networks.

[bookmark: _heading=h.30j0zll]PART II – PRODUCTS

2.01 MANUFACTURER
[bookmark: _Hlk152857477]Basis of design: Horton Automatics, a division of Overhead Door Corporation, shall manufacture automatic sliding door(s) of type(s) and size(s) specified on plans and door schedule. 2501 S. State Hwy TX-121 Business Suite 200, Lewisville, TX 75067 Toll Free: 800-531.3111 www.hortondoors.com. specs@hortondoors.com 

☐.[Substitutions:  Requests for substitution and product approval in compliance with the specifications must be submitted in writing and in accordance with the procedures outlined in Division 1, Section “Substitution Procedures”.  Approval of requests is at the discretion of the architect, owner, and their designated consultants.]

🗹.[Substitutions:  Not Permitted]

[bookmark: _heading=h.1fob9te]2.02 EQUIPMENT
A. Dimensions: {CHOOSE 1}

· Exact Dimensions:
Enter Unit Width: 
      	Enter Unit Height [to top of the header]:

· Follow door schedule	
 2.02.01. DOOR ASSEMBLIES
A. MANUFACTURED DOOR UNITS: Shall include operator, header with roller track, carrier assemblies, framing, sliding door panel(s), sidelite(s), activation, safety devices and accessories required for complete installation. 
1. [bookmark: _heading=h.3znysh7]Configuration: Bi-parting

2. Mounting Type:
· Perimeter mounted within rough opening with sliding panel(s) sliding along sidelite. 
3. Door Type: Type 110: Slide-swing panel(s) ‘SX’ shall slide along exterior side.

B. DEFINITIONS
1. SO panel: stationary sidelite capable of swinging away for emergency egress
2. SX panel: sliding panel capable of swinging away for emergency egress
3. O panel: a fixed panel with no capability to either slide or swing away
4. Single Slide: a door system with one stationary panel and one moving panel that open/closes on one side. The moving and stationary panels overlap when the door is open.
5. Bi-Parting Slide: a door system with two moving panels that slide in opposite directions with two stationary panels that overlap the slide panels when the door is open 
6. [bookmark: _heading=h.2et92p0]Type 010 – non breakout: Sliding panel(s) ‘X’ shall slide along interior side.
7. Type 110 – partial breakout: Slide-swing panel(s) ‘SX’ shall slide along exterior ‘O’ fixed sidelite(s).
8. Type 310 – full breakout: Slide-swing panel(s) ‘SX’ shall slide along interior ‘SO’ swing-out sidelite(s)

2.02.02 DOOR OPERATOR AND CONTROLLER
A. OPERATOR:
1. [bookmark: _heading=h.tyjcwt]The Electric Operating Mechanism shall be HD-Slide® Series 2001 6” x 8” Header
2. The operator shall be mounted and concealed within the header.
3. On/Off Switch shall be supplied. When switched OFF or during electrical power failure, the unit reverts to free manual operation.
4. Operating force shall be accomplished through a 1/4 HP DC permanent magnet motor with worm gear transmission and 1800 RPM working with a drive belt, attached door hangers, and idler pulley.
5. Drive belt to be 1" (13 mm) wide.
6. Idler pulley to be reinforced, metallic material.
7. Maximum current draw shall not exceed 3.15 Amps
8. {CHOOSE 1: 120VAC OR 240VAC} , single-phase, dedicated 20 Amps circuit per operator.

B. MASTER CONTROL:
1. The controller shall be a 16-bit microprocessor with dual on-board seven-segment alphanumeric diagnostic display and position encoder.
2. The encoder shall monitor revolutions of the operator shaft and send signals to the microprocessor controller to define door position and speed.
3. [bookmark: _heading=h.3dy6vkm]The control shall have minimum of 28 programmable parameters including the following functions as required by ANSI A156.10:
a. 	Adjustable opening and closing speeds.
b.	Adjustable back-check and latching.
c.	Adjustable braking.
d.	Adjustable hold-open time between 1 to 30 seconds.
e.	Adjustable Reversing Circuit will reopen door unit if closing path is obstructed.
f.	Separate day and night modes of operation with security over-ride.

2.02.03 COMPONENTS
A. HEADER: 
1. [bookmark: _heading=h.1t3h5sf]The header shall have a removable face plate for service and adjustment of the operator and controls.
2. Header Capacity:
Bi-Parting: Up to 300 lbs. (113.4 kg) per slide panel over spans up to 16’-0” (4877mm) without Single Slide: Up to 500 lbs. (113.4 kg) per slide panel over spans up to 9’-0” (2743mm) without intermediate supports.

B. CARRIER ASSEMBLIES AND HEADER ROLLER TRACK:
1. Carrier assemblies shall support door panels with a minimum of four rollers per panel.
2. Rollers will be Acetal Ball bearing wheels 2" (51 mm) diameter. 
3. Anti-Derailing (anti-raise) shall be accomplished by means of a continuous aluminum extrusion full length of slide panel travel. The overhead header roller track shall be continuous aluminum.

C. SLIDING PANEL(S) AND SIDELITE(S):
[bookmark: _heading=h.4d34og8]Minimum door panel extrusion wall thickness Default: 0.125”
1. Stile: Shall be aluminum: Medium stile construction: 3 3/4” (95mm) wide.

2. [bookmark: _Hlk148360354]Muntin Bar:  An intermediate horizontal rail shall be furnished for safety and division of glass 
{CHOOSE 1}
2-1/4" (57 mm) (default)
No muntin
3. [bookmark: _heading=h.2s8eyo1]Bottom rail:  Shall be {CHOOSE 1}:
6 1/2" (165 mm)
8" (203 mm)
10" (254 mm) (default)
4. Sliding panels shall have concealed bottom guides to stabilize slide travel.
5. Weather-stripping: Along perimeter of sliding panel(s) and swing-out sidelite(s). Weatherstripping material captured in extruded aluminum door panel. Surface applied self-adhesive weatherstripping not acceptable. Adjustable spring-loaded double astragal weather-stripping at lead edge, double mohair at interlock rails.
6. Finger Safety: Strike rail of sliding panel will stop short of adjacent sidelite.
7. Weight Limit: The total weight limit per panel shall be 500 lbs. for the UL listed slide-swing panel.

D. BREAKOUT PANELS:
1. Slide-swing panels can swing out a minimum of 90° from any position of slide movement and require no more than 50 lbf. (222 N) of force applied at the lock stile to open.
2. Slide-swing panels and swing-out sidelites shall utilize a spring-loaded ball detent and shall have a torsion spring designed to re-close the panel if pushed open in the direction of egress without user intervention.
3. The breakout mechanism shall provide support across the full width of the door in normal operating mode. In breakout mode, the torsion assembly shall support the weight of the door to minimize drop during emergency egress.
4. Slide-swing panels shall include an intermediate horizontal rail.
5. Units with a breakout feature are ETL listed as an exit away and are compliant with NFPA 101.

E. JAMBS/FRAME: Shall be aluminum:
[bookmark: _heading=h.17dp8vu]1 3/4" (44mm) deep x 4 (104 mm) high (default)
Frame Option: Transom of size and type indicated, mounted on the header.

F.  THRESHOLD: Shall be aluminum:
1/2” (13mm) tall by 7” (178mm) wide

G. HARDWARE: 
1. [bookmark: _heading=h.3rdcrjn]Standard lock: ANSI A156.5, Grade 1, 2-Point Locking provided and installed in the strike rail shall include:
a. Hookbolt Latch, 5/8” laminated stainless steel, latching into jamb or adjacent strike rail.
b. 3/8” hex-bolt into breakout carrier frame.
c. Keyed 1 5/32" (29 mm) Cylinder mounted on the exterior side with 31/32" (25 mm) backset.
d. Thumbturn mounted on the interior side.
e. 3/8” Lockbolt extending 1/2” into breakout carrier frame and threshold.
2. Automatic lock: Automatically locks slide function of door when in closed position. Additional power supply for autolock is not acceptable. {CHOOSE 1}:
Autolock Fail Secure: If power fails the lock engages
Fail Safe Autolock: Autolock Fail Safe: If power fails the lock disengages.
No Autolock

H. GLASS AND GLAZING: 
Glass stops, glazing vinyl and setting blocks for field glazing as per Safety Glazing standard ANSI Z97.1.2. Glazing prep to be for 1” UL752 BR-3 rated glass as specified by the manufacturer.

I. POWER FAIL OPTION:
1. [bookmark: _heading=h.lnxbz9]Monitored Power Fail (battery back-up) {CHOOSE 1}:
Power Fail Open (Fail Safe): If power fails the door slides open
Power Fail Close (Fail Secure): If power fails the door slides closed
No Power Fail

2.02.04 ACTIVATION AND SAFETY:
1. AUTOMATIC ACTIVATION. Shall be 24 VDC, class ll circuit and shall be adjusted and installed in compliance with ANSI A156.10. The system shall include the following:
1. ACTIVATION SENSORS: Microwave or active infrared sensors shall be header-mounted on each side of the door unit for detection of traffic from each direction. 
2. THRESHOLD MONITORED PRESENCE SENSORS:
· Header-mounted sensors shall provide active infrared presence detection on each side of the door unit and shall remain active throughout the entire door opening and closing cycle. 
· Hold-open beams: Two pulsed infrared photoelectric beams to be mounted in vertical rails of sidelite or in jambs. Sender/receiver arrangement parallels door opening.
2.02.05 MATERIALS, FINISHES, AND FABRICATION EXTRUDED ALUMINUM:
A. EXTRUDED ALUMINUM: ASTM B221, 6063-T5 alloy and temper, anodized:
1. 	Structural Header Sections: Minimum 3/16" (5 mm) thickness.
2. 	Structural Frame Sections: Minimum 1/8" (3 mm) thickness.
3. 	Structural Panel Sections: Minimum 1/8" (3 mm) thickness.
[bookmark: _heading=h.35nkun2]
[bookmark: _heading=h.1ksv4uv][bookmark: _Hlk152857526]B. FINISH {CHOOSE FROM 1, or 2}
1. If Anodize Finish {CHOOSE 1}:
· 204-R1 Clear: Architectural Class 1 Clear Anodized Coating, AA-MI2C22A31.
· Champagne: Architectural Class 1 Anodized Coating, AA-MI2C22A44.
· 311-R1 Light Bronze: Architectural Class 1 Anodized Coating, AA-MI2C22A44.
· 312-R1 Medium Bronze: Architectural Class 1 Anodized Coating, AA-MI2C22A44.
· 313-R1 Dark Bronze: Architectural Class 1 Anodized Coating, AA-MI2C22A44.
· Black: Architectural Class 1 Anodized Coating, AA-MI2C22A44.
2. If Paint finish {CHOOSE 1}:
1. Powder Coat: 100% V.O.C. free fluoropolymer resin based. Color Code TBD.
2. Wet Paint: Color Code TBD.

C.	PANEL CONSTRUCTION: 	
1.	Corner block type with 3/16” steel backup plate construction, mechanically secured with minimum of four hardened steel screws and threaded rod reinforcement. Vertical rails to have reinforcing A36 steel backup tube: 1” square x 1/8”, full length of vertical rail. Sash consists of snap-in glass stops, snap-in glazing beads and vinyl gaskets. Unlike common thru-bolt designs, corner blocks prevent distortion of the door panels during use and abuse.
2.	Slide-swing doors to be supplied with adjustable glass setting block to allow for adjusting of door to meet site conditions eliminating the need for additional shims. 
3.	Adjustable double astragal with dual weatherstrip physically captured for superior seal standard (adhesive applied weatherstrip not acceptable) 

D.  FRAME CONSTRUCTION: Butt joints, mechanically secured with screws and formed alum. corner brackets.

E.  OPERATOR CONSTRUCTION: Electromechanical, modular type construction.

PART III - EXECUTION
3.01 EXAMINATION
SITE VERIFICATION OF CONDITIONS:
1. The installer shall verify that the base conditions meet the manufacturer's instructions for product installation. Any negative conditions that may affect the proper and timely completion of work must be notified to the Contractor in writing. All negative conditions must be corrected in a manner acceptable to the manufacturer.
2. With the installer present, examine doors and frames for compliance with installation tolerances, wall and floor construction, and other conditions affecting performance.
3. Verify the actual locations of wiring connections for roughing-in electrical source power.
4. The installer must correct all unsatisfactory conditions before proceeding with the installation.
3.02 INSTALLATION 
A. ENTRANCES: 
Install automatic entrances plumb and true in alignment with established lines and grades without warp or crack of framing members and doors. Use concealed fasteners to the greatest extent possible for surface-mounted hardware. Set headers, carrier assemblies, tracks, operating brackets, and guides level and true to location with anchorage for permanent support.

B. DOOR OPERATORS: 
Connect door operators to the electrical power distribution system as specified in Division 26 Sections.

C. GLAZING: 
Install glazing according to the automatic door manufacturer's instructions, the Glass Association of North America (GANA) Glazing Manual, and glass product manufacturer recommendations.

D. SEALANTS: 
Use sealants to comply with the requirements specified in Division 7 Section "Joint Sealants" to provide a weather-tight installation. Set thresholds, bottom guide and track systems, and framing members in full bed of sealant.

E. DISSIMILAR MATERIALS: 
Separate aluminum materials and other corrodible surfaces from sources of corrosion or electrolytic action contact points to comply with AAMA 101, Appendix Dissimilar Materials.

3.03 CLEANING, ADJUSTMENT, AND PROTECTION
A. CLEANING AND ADJUSTMENT: 
1. Remove temporary protection of adjacent work areas. Remove construction debris from construction sites and legally dispose of debris. Repair or replace damaged installed products. Clean product surfaces and lubricate operating equipment for optimum condition and safety.
2. Adjust door operators, controls, and hardware for smooth and safe operation in compliance with ANSI/BHMA A156.10.
3. Verify installation and alignment of all entrance weatherstripping as required.

B. ADVISE CONTRACTOR: Of precautions required throughout the remainder of the construction period, to ensure that doors will be without damage or deterioration (other than normal weathering) at the time of acceptance.

3.04 FIELD QUALITY CONTROL
The manufacturer’s representative shall provide technical assistance and guidance for the installation of automatic doors. Factory trained and AAADM certified representatives shall test and inspect each automatic door to determine compliance of the installed system to ANSI/BHMA A 156.10.

3.05 INSTRUCTION
Following the installation and final adjustments, the installer shall fully instruct the facility manager as to the correct operating procedure and safety requirements of the sliding door package.

END OF SECTION

Horton Automatics reserves the right to make product improvements and change specifications without notice.
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