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DIVISION 08 - OPENINGS | SECTION 08 42 33 
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AUTOMATIC SLIDING ENTRANCES
EasyFlow® [MANUAL or POWER ASSISTED] Revolving Door – Diameter 6’ - 10’
Automatic Revolving Doors | F14.1


	[bookmark: _Hlk152857433]Specification
	Selection

	Door ID
	{Door_ID}

	Product name {Choose 1}
Section 2.02 A 
	EasyFlow® Manual Series 9531 – 3-Wing with Segmented Drum [Diam 6’ – 8’]
EasyFlow® Manual Series 9530 – 3-Wing with Round Drum, [Diam 6’ – 8’]
EasyFlow® Manual Series 9541 – 4-Wing with Segmented Drum [Diam 6’ – 8’]
EasyFlow® Manual Series 9540 – 4-Wing with Round Drum, [Diam 6’ – 8’]
AutoFlow® Power Assisted Series 9931 – 3-Wing with Segmented Drum [Diam 6’ – 10’]
EasyFlow® Manual Series 9930 – 3-Wing with Round Drum, [Diam 6’ – 10’]
EasyFlow® Manual Series 9541 – 4-Wing with Segmented Drum [Diam 6’ – 10’]
EasyFlow® Manual Series 9540 – 4-Wing with Round Drum, [Diam 6’ – 10’]

	Diameter
	Per door schedule or TBD

	Height (to top of roof)
	Per door schedule or TBD

	Design
	Edit Section 2.02 I 1 & 2

	Finish
	Edit Section 2.04 B 1 & 2 & 3

	Security Options
	Edit Section 2.02 C 2

	Canopy
	Edit Section 2.02 I 3

	Drum and Wings
	Edit Section 2.02 J

	Voltage
	Edit Section 2.03 A

	Applicable codes
	ANSI 156.27, ANSI Z97.1, UL325, AAADM




These specifications represent the exacting selection you have made for your project {PROJECT}, including door configuration, colors and options and depict design features that are commonly used. Horton Automatics will custom manufacture each product to these specifications. It is the customer’s responsibility to validate that each configuration is suitable for the intended application. All specifications and designs contained herein are subject to change without notice or obligation. Consult www.hortondoors.com’ spec desk at 1-800-531-3111 or specs@hortondoors.com for assistance.



DIVISION 08 - OPENINGS
SECTION 08 42 33 - REVOLVING DOOR ENTRANCES


PART I – GENERAL

1.01 SUMMARY

A. 	WORK INCLUDED: Furnish complete manual aluminum revolving door system, as specified, that has been manufactured, fabricated, and installed to maintain performance criteria stated by manufacturer without defects, damage, or failure.

B. 	RELATED WORK:
1. 	Openings: Division 08, applicable sections.
2. 	Electrical: Division 26, applicable sections.

1.02 REFERENCES

A.  AMERICAN ASSOCIATION OF AUTOMATIC DOOR MANUFACTURERS (AAADM).

B.	AMERICAN ARCHITECTURAL MANUFACTURERS ASSOCIATION (AAMA) 101: Appendix Dissimilar Materials.	

C. 	AMERICAN NATIONAL STANDARDS INSTITUTE (ANSI):
1. 	ANSI 156.27: Power and Manual Operated Revolving Pedestrian Doors
2. 	ANSI Z97.1: Safety Glazing Materials Used in Buildings - Methods of Test.

D. 	AMERICAN SOCIETY FOR TESTING AND MATERIALS (ASTM) B221: Aluminum-Alloy Extruded Bars, Rods, Shapes and Tubes.

E. 	THE ALUMINUM ASSOCIATION (AA): Aluminum Finishes Manual

[bookmark: _Hlk110244792]F. 	INTERTEK, WARNOCK HERSEY (ETL): Testing Laboratory and Certification Agency joined with ETL SEMKO  

G. 	UNDERWRITERS LABORATORY, INC. (USA & CANADA) UL 325: Electrical Door, Drapery, Gate, Louver, and Window Operators and Systems.

1.03 SUBMITTALS

A. 	SHOP DRAWINGS & PRODUCT DATA: Submit drawings and product data showing layout, profiles, product components including anchorage, accessories, finish and glazing details (where required).

B. 	QUALITY ASSURANCE AND CLOSEOUT SUBMITTALS: Submit the following:
1. 	Owner’s Manual & Warranty document as specified herein.
2. 	AAADM inspection compliance form completed and signed by certified AAADM inspector prior to doors being placed in operation as proof of compliance with ANSI A156.27.

1.04 QUALITY ASSURANCE

A. 	INSTALLERS QUALIFICATIONS: Installer shall be factory trained, certified by AAADM, and experienced to perform work of this section.

B. 	MANUFACTURER’S QUALIFICATIONS: Manufacturer to have minimum (5) five years successful experience in the fabrication of manual doors of the type required for this project. Manufacturer capable of providing field service representation during installation, approving acceptable installer, and approving application method.

1.05 WARRANTIES

A. 	MANUFACTURER'S WARRANTY: Units to be warranted against defect in material and workmanship for a period of two years from the Date of Substantial Completion. Manufacturer's warranty is in addition to, and not a limitation of, other rights owner may have under Contract Documents.

B. 	DISTRIBUTOR'S WARRANTY: One-year warranty: Labor & transportation charges for defective parts replacement. Three-year Distributor’s Warranty for electronic speed control.

1.06 PROJECT CONDITIONS

FIELD MEASUREMENTS: Verify actual dimensions/openings by field measurements before fabrication and record on shop drawings. Coordinate with fabrication and construction schedule to avoid construction delays.

1.07 DELIVERY, STORAGE AND HANDLING

A. 	ORDERING AND DELIVERY: Comply with factory's ordering instructions and lead time requirements. Delivery shall be in factory's original, unopened, undamaged containers with identification labels intact.

B. 	STORAGE AND PROTECTION: Provide protection from exposure to harmful weather conditions and vandalism.

PART II – PRODUCTS

2.01 MANUFACTURER

HORTON AUTOMATICS, a division of Overhead Door Corporation, shall manufacture manual revolving door(s) of type(s) and size(s) specified on plans and door schedule.

2.02 EQUIPMENT
DIMENSION: {CHOOSE 1}
· Exact Dimensions:
Enter Width [opening width minus ½”]:
      	Enter Height [to top of the header}
· Follow door schedule
A. MANUFACTURED DOOR UNITS: Shall be {CHOOSE 1}
EasyFlow® Manual Series 9531 – 3-Wing with Segmented Drum [Diam 6’ – 8’]
EasyFlow® Manual Series 9530 – 3-Wing with Round Drum, [Diam 6’ – 8’]
EasyFlow® Manual Series 9541 – 4-Wing with Segmented Drum [Diam 6’ – 8’]
EasyFlow® Manual Series 9540 – 4-Wing with Round Drum, [Diam 6’ – 8’]
AutoFlow® Power Assisted Series 9931 – 3-Wing with Segmented Drum [Diam 6’ – 10’]
EasyFlow® Manual Series 9930 – 3-Wing with Round Drum, [Diam 6’ – 10’]
EasyFlow® Manual Series 9941 – 4-Wing with Segmented Drum [Diam 6’ – 10’]
EasyFlow® Manual Series 9940 – 4-Wing with Round Drum, [Diam 6’ – 10’].

B. [bookmark: _Hlk38293553]SPEED CONTROL {CHOOSE a OR b BASED ON YOUR SELECTION ABOVE}
a. SERIES 9500:  Precision machined steel casting overhead speed control with precision machined 100:1 ratio gear train, steel case, adjustable and replaceable brake blocks. Speed Control shall be limited up to 12 RPM (refer to ANSI standard 156.27) and provide smooth and effective braking action. 
b. SERIES 9900  Speed Control: Shall be limited up to 2 RPM (refer to ANSI standard 156.27) and provide smooth and effective braking action. Automatic Home Positioning Drive System: Motion sensor unlocks brake and allows for wing rotation after pedestrian pushes door wing. Rotation stops at optimal position

[bookmark: _Hlk38293611]C. 	COLLAPSING MECHANISM: Door design shall be equipped with mechanical breakaway and completely bookfold in case of emergency as required by Codes. Wings can be broken away with 80-130 lbs. (355-578 N) of force (adjustable).

D. 	ENCLOSURE: Shall be extruded aluminum and glass/glazing material and shall be constructed maintaining proper clearances and weather seal. {CHOOSE 1}
1. Segmented® Design:
2. Round Design
3. 	Canopy: Standard canopy be shall round and minimum 4” (102mm) high. Interior ceiling shall be 3/4” thick plywood laminated with .060” (1.5mm) aluminum to match door finish. . {CHOOSE 1}
1. Segmented® Design:
2. Round Design
4. Canopy options shall include: {CHOOSE THOSE THAT APPLY}
a. 	Extended canopy {ADD HEIGHT}
b. 	Cropped canopy [exterior]
c. 	Cropped canopy [interior]
d. 	Exterior roof fabricated from .090" (2mm) anodized aluminum. 
e. 	Two ceiling lights with energy efficient lighting systems with flush lens.  

E. 	PANEL/DOOR WING: 
1. Narrow
2. Medium
3. Wide	
· Perimeter weather-stripping utilizing affixed sweeps shall ensure weather seal. Standard glazing prep to be for 1/4” (6 mm) glass/glazing material and shall have sloped stops on horizontal rails (except on clad units). An intermediate surface applied horizontal flat aluminum push bar, 3/8” (10mm) thick x 1 ½” (38mm) wide, shall be furnished for each wing for safety. 
· Door Wing options shall include: {CHOOSE THOSE THAT APPLY}
1. 	Stainless steel or brass flat push bars.
2. 	Round push bars: 1” (25mm) diameter, aluminum, stainless steel or brass 
3. 	Horizontal muntins (mid-rails): 2 ¼” (57mm) or 4” (102mm) wide.
4. 	Optional bottom rails: 6 ½” (165mm) (standard for medium stile), 8” (203mm), or 10” (254mm).
5. 	Medium stile rails (standard for diameters 8’-0” and over) 
6. 	Prep for glazing up to 1" (25mm).
7. 	Fixed wings. (Must be approved by the authority having jurisdiction)

F. 	HARDWARE: Provided shall include:
1. 	Locks with five pin cylinders and concealed bolts provided on two door wings.
2. 	Bottom pivot/bearing: Surface mounted with no excavation below floor line required.
3. 	Center Shaft: 1-1/2” (38mm) diameter steel shaft with connections to speed control and bottom pivot/bearing.

2.03 RELATED WORK REQUIREMENTS
 
A. 	ELECTRICAL: (for optional ceiling lights) {CHOOSE 120VAC or 240VAC], 60 cycle, single phase, 20 amp in conduit routed to canopy.

B. 	GLASS AND GLAZING: Glass stops, glazing vinyl and setting blocks for field glazing as per Safety Glazing standard ANSI Z97.1.2. General contractor to coordinate acquisition of glass, not already provided by manufacturer, in thickness and type in accordance with manufacturer's recommendations for prescribed design.
1. 	Door Wing Glazing: (provided by others): 1. {CHOOSE 1}   
a.   Standard flat safety glass in clear, 1/4” (6mm) tempered
b.	1/4” (6mm) clear tempered glass
c.	7/16” (11mm) laminated glass with Solar Blue, Grey or Bronze tint
d.	7/16” (11mm) Starphire Low Iron laminated glass  
e.	9/16” (14mm) clear laminated glass
f.	9/16” (14mm) Starphire Low Iron laminated glass  
2. 	{IF SEGMENTED ENCLOSURE SELECTED, CHOOSE 1} 
a.   Standard flat safety glass in clear, 1/4” (6mm) tempered
b.	1/4” (6mm) clear tempered glass
c.	7/16” (11mm) laminated glass with Solar Blue, Grey or Bronze tint
d.	7/16” (11mm) Starphire Low Iron laminated glass  
e.	9/16” (14mm) clear laminated glass
f.	9/16” (14mm) Starphire Low Iron laminated glass  

 3. Round Enclosure Glazing: (provided by factory) Standard material will be curved safety glass {CHOOSE 1}
a.	1/8” (3mm) aluminum 
b.	1/4” (6mm) clear tempered glass
c.	7/16” (11mm) laminated [STANDARD]
d.   7/16” (11mm) laminated glass with Solar Blue, Grey or Bronze tint
d.	7/16” (11mm) Starphire Low Iron laminated glass  
e.	9/16” (14mm) clear laminated glass
f.	9/16” (14mm) Starphire Low Iron laminated glass  

2.04 MATERIALS, FINISHES AND FABRICATION

A. 	EXTRUDED ALUMINUM: ASTM B221, 6063-T5 alloy and temper, anodized:
1. 	Structural Drum/Enclosure Sections: Minimum 1/8" (3mm) thickness.
2. 	Structural Panel/Door Wing Sections: Commercial grade.

B. FINISH {CHOOSE 1, 2 OR 3}
1. Anodize finish: {CHOOSE 1}
1. 204-R1 Clear: Arch. Class 1 Clear Anodized Coating, AA-MI2C22A31.
2. Champagne: Arch. Class 1 Anodized Coating, AA-MI2C22A44.
3. 311-R1 Light Bronze: Arch. Class 1 Anodized Coating, AA-MI2C22A44.
4. 312-R1 Medium Bronze: Arch. Class 1 Anodized Coating, AA-MI2C22A44.
5. 313-R1 Dark Bronze: Arch. Class 1 Anodized Coating, AA-MI2C22A44.
2. Paint Coating: {CHOOSE 1}
· Powder Coat: 100% V.O.C. free fluoropolymer resin-based. Color: {color}.
· Wet Paint. Color: {color}
3. Clad finish WINGS & ROUND DRUM ONLY: {CHOOSE 1}
· Stainless Steel #4 (Satin Finish): Architectural Satin Finish Clad Coating.
· Stainless Steel #8 mirror finish (Reflective): Architectural Reflective Clad Coating.
· Bronze #4 (Satin Finish): Architectural Satin Finish Clad Coating.
· Bronze with polish, non-directional finish: Architectural Non-Directional Polished Clad Coating.
· Brass #4 (Satin Finish): Architectural Satin Finish Clad Coating.
· Brass with a polished, non-directional finish: Architectural Non-Directional Polished Clad Coating.
· Muntz metal (brass alloy): Architectural Clad Coating.

C. 	DOOR WING CONSTRUCTION: 
1.	Corner block type with 3/16” steel backup plate construction, mechanically secured with minimum of four hardened steel screws. Sash consists of snap-in glass stops, snap-in glazing beads and vinyl gaskets. 
2.	Weather-stripping material captured in extruded aluminum door panel. Surface applied self-adhesive weather-stripping not acceptable.

D. 	ENCLOSURE CONSTRUCTION: Butt joints, mechanically secured by means of screws and formed aluminum corner brackets.

PART III - EXECUTION

3.01 EXAMINATION

SITE VERIFICATION OF CONDITIONS: Installer must verify that base conditions previously installed under other sections are acceptable for product installation according to with manufacturer's instructions. Notify the Contractor in writing of conditions detrimental to the proper and timely completion of work. Do not start work until all negative conditions are corrected in a manner acceptable to the installer and manufacturer.

3.02 INSTALLATION

A. 	GENERAL: Install door unit(s) plumb, level and true to line, without warp or rack of enclosure. Drum enclosure can be center connected to adjacent construction or 'throat connected' (at entry vertical rails). Allow for 1/4" shim space each side and at canopy. Anchor in place. Unit is free-standing with no additional support required. Adjacent construction not to bear down on revolving door. 

B. 	DISSIMILAR MATERIALS: Comply with AAMA 101, Appendix Dissimilar Materials by separating aluminum materials and other corrodible surfaces from sources of corrosion or electrolytic action contact points.

C. 	WEATHER-TIGHT CONSTRUCTION: Install enclosure with joint filler or gaskets and sealant. Coordinate installation with wall flashings and other components of construction. 

D. 	ELECTRICAL: General or electrical contractor to install all wiring to optional equipment on a separate circuit breaker routed into canopy.

3.03 CLEANING, ADJUSTMENT AND PROTECTION

A. 	CLEANING: After installation, installer to take following steps:
1. 	Remove temporary protection of adjacent work areas. Remove construction debris from construction site and legally dispose of debris.
2. 	Repair or replace damaged installed products. Clean product surfaces and lubricate operating equipment for optimum condition and safety.

B. 	ADVISE CONTRACTOR: Of precautions required through the remainder of the construction period, to ensure that doors will be without damage or deterioration (other than normal weathering) at the time of acceptance.



END OF SECTION

Horton Automatics reserves the right to make product improvements and change specifications without notice.
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